Gemplus GemPC410 / GemPC410-FD /GemPC410-SL Smart Card Interface
drivers disk for Windows Server 2003.
Version 2.6.3, june 2003.


Caution:
--------
This readme file is specifically written for the afore-mentioned 
driver version. Before proceeding, you might want to check whether a
later driver version is available from the Gemplus web site 
(http://www.gemplus.com/).


Contents:
---------

   1. Release notes
   2. Pre-Requisites
   3. Disk Content
   4. Smart Card Interface driver use
   5. User notes (Known deviations)
   6. Troubleshooting
   7. Support


1. Release notes
----------------
Version 2.6.3:
	Add Support to pass the WHQL on server 2003.

Version 2.6.1 :
   TimeOut IOCTL improvement

Version 2.6 :
   Version for Case.

Version 2.0.10:
   This is the first version fully compatible with Microsoft
   Windows Server 2003.
   It is specifically designed for GemCore 1.21 firmware.
   It fixes some problems with:
    * RING signal
    * TimeOut IOCTL
    * Case 4 with 256 data bytes
    * MaximumBaudRate registry key

Version 2.0.2:
   It is specifically designed for GemCore 1.21 firmware.
   The driver name was changed to avoid a conflict with 
   Microsoft Windows Server2003 (2.0.0)
   It fixes a problem with the version provided on the 
   Windows 2000 CD.

Version 1.1.0:
   It is specifically designed for GemCore 1.21 firmware.
   It provides the following new features:
    * New Vendor attributes IOCTL (1.0.6)
    * Switch Speed IOCTL (1.0.5)
    * Communication resets to 9600 bauds when the device is
      stopped (1.0.3)
    * Masked version support for customized devices (1.0.2)
   It fixes some problems with:
    * Reader removal / insertion when a smart card is 
      present (1.0.4)

Version 1.0.0:
   Driver for serial readers with firmware version 1.118
   or above, and compliant with PnP.


2. Pre-Requisites
-----------------

To be able to conduct the following action, you need to have
Administrator privilege on the workstation.

To be usable, this installation requires that the Microsoft Smart Card 
Manager be started.

Note: All Microsoft Smart Card Manager components are already 
installed with Windows Server 2003. 
DO NOT INSTALL THE SCBASE.EXE OR SMCLIB.EXE COMPONENTS even though 
they might be part of this distribution.

To check the status of the Microsoft Smart Card Manager:
   * Start the Computer Management Console by right-clicking on the 
   "My Computer" desktop icon and pick the "Manage" item in the menu,
   * Select and open the "Services and Application" group in the list,
   * Click on the "Services" item,
   * Double-click on the "Smart Card" service.
   * The service status should be "Started" 

   If this is not the case,
   * Choose "Automatic" in the "Startup Type" drop-down list, then
   * click on the <Apply> button to start the service.

   You can now close the Computer Management Console.

In the rest of this file, we assume that you know how to start the
Device Manager. To do so:
   * Right-click on the "My Computer" desktop icon and pick the 
   "Properties" item in the menu.
   * Select the "Hardware" tab and click on the <Device Manager...>
   button


3. Disk Content
---------------

The following components are included with this Disk:
   - Readme.txt   Ver 2.6.0              24/05/2002
     This file.
   - GemSer.Sys	  Ver 2.6.0              25/04/2002
     PC/SC driver for Gemplus Smart Card Interface
   - GemSer.inf	  Ver 2.0.10             25/04/2002
     Installation file for Microsoft Wizard
   - GemSer.Cat  
     Signature File from MS Windows Hardware Quality Labs


4. Smart Card Interface driver use
-----------------------------------

   4.1. Driver installation

   WARNING: the reader power cable must not be connected to the 
   keyboard port when the computer is running, this action may
   damage your machine!
   Power off the PC before any operation on that connector!

      4.1.1. Installation

         As Windows Server 2003 come with a limited version of this driver, 
         installation should be done in two phases.
         The first one installs the default driver,
         the second one updates the system with this new driver.
 
         Install the default driver:
         Power off the computer.
         Connect your reader as shown on the Reader carton.
         Remove any floppy disk and restart your system.
         Wait for Windows to install the default device driver.

         Update the system:
         Right-click on the "My Computer" icon on the desktop,
         Choose "Properties" and select the "Hardware" tab,
         Press the <Device Manager> button,
         Select the "Smart card readers" group,
         Double-click on "GEMPLUS GemPC410P Serial Smart Card Reader"
         Select the "Driver" tab
         Click on <Update Driver>
         Click <Next>
         Select "Display a list of the known drivers for this device 
         so that I can choose a specific driver", and click <Next>
         Click <Have Disk...>
         Browse to the driver files location (the "WinServer2003" directory
         within the folder where you unpacked the archive) and 
         click <OK>
         Select "GEMPLUS GemPC410P Serial Smart Card Reader", and 
         click <Next>
         The Wizard is ready to install the driver, click <Next>.
         Click <Finish> to close the Microsoft Device Driver Wizard.

      4.1.2. Check your installation

         Open the Device Manager.
         Double-click on "GEMPLUS GemPC410P Serial Smart Card Reader"
         in the "Smart card readers" group
         Select the "Driver" tab
	 Check that the "Driver version" matches the one for this file.

   
   4.2. Driver update

      4.2.1. Update

         Right-click on the "My Computer" icon on the desktop,
         Choose "Properties" and select the "Hardware" tab,
         Press the <Device Manager> button,
         Select the "Smart card readers" group,
         Double-click on GemPC410 target reader
         Select the "Driver" tab
         Click on <Update Driver>
         Click <Next>
         Select "Display a list of the known drivers for this device 
         so that I can choose a specific driver", and click <Next>
         Click <Have Disk...>
         Browse to the driver files location (the "WinServer2003" directory
         within the folder where you unpacked the archive) and 
         click <OK>
         Select "GEMPLUS GemPC410 Serial Smart Card Reader", and 
         click <Next>
         The Wizard is ready to install the driver, click <Next>.
         Click <Finish> to close the Microsoft Device Driver Wizard.


      4.2.2. Check your update

         Right-click on the "My Computer" icon on the desktop,
         Choose "Properties" and select the "Hardware" tab,
         Press the <Device Manager> button,
         Select the "Smart card readers" group,
         Double-click on GemPC410 target reader
         Select the "Driver" tab
	 Check that the "Driver version" matches the one for this file.



   4.3. Driver removal

   WARNING, the reader power cable must not be disconnected from the 
   keyboard port when the computer is running, this action may
   damage your machine!
   Power off the PC before any operation on that connector!

      4.3.1. Removal

         Right-click on the "My Computer" icon on the desktop,
         Choose "Properties" and select the "Hardware" tab,
         Press the <Device Manager> button,
         Select the "Smart card readers" group,
         Double-click on the GemPC410 target reader
         Click on the <Uninstall> button in the toolbar, or select the
	 "Uninstall..." item from the "Actions" menu.
         When prompted, confirm the operation by clicking <OK>
         When this operation is finished, power off the computer and
         disconnect the reader 


      4.3.2. Check the removal
         
         Right-click on the "My Computer" icon on the desktop,
         Choose "properties" and select the "Hardware" tab,
         Press the <Device Manager> button,
         Select the "Smart card readers" group,
         Verify that no "GEMPLUS GemPC410P Serial Smart Card Reader" 
         appears any longer.


5 - User notes (known deviations)
---------------------------------


6. Troubleshooting
-------------------

If the previously described procedure didn't succeed in installing or
updating the driver, please

1- Verify that the reader cable is connected to a usable computer
   COM port

2- Verify that the power cable of the reader is connected to
the keyboard port.

3- Open the Device Manager, 
   click on the "Smart card readers" group and
   check the state of the "GEMPLUS GemPC410P Serial Smart Card Reader".
   If a cross appears, right-click on the reader entry, 
   select "Properties" in the menu,
   select "Do not use this device in any hardware profile"
   in the "Device usage" drop-down list then
   contact the support.


7. Support
----------

In case of problem, please contact Gemplus through the Gemplus web site 
(http://www.gemplus.com/) or depending on your location :

For North America
	email : HOTLINEUSA@gemplus.com
	tel +1 (877) 436-7233

For ASIA
	email : ASIA.hotline@gemplus.com
	No phone line

For other countries
	email : hotline@gemplus.com
	tel +33 (0) 442 36 50 50

----------------------------------------------------------------------